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Table S1. Source water quality analysis.
	Parameter
	Reported Value

	pH
	7.4

	Alkalinity
	274 mg/L as CaCO3

	Fluoride
	0.7 mg/L

	Orthophosphate
	0.5 mg/L

	Free Ammonia
	0.09 mg/L

	Nitrate
	1.1 mg/L

	Nitrite
	0.009 mg/L

	Sulfate
	70 mg/L

	Calcium
	300 mg/L as CaCO3

	Magnesium
	124 mg/L as CaCO3

	Hardness
	424 mg/L as CaCO3
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Figure S1. Time-course monitoring of free chlorine, total chlorine and ORP at the studied pool facility.
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[bookmark: _Hlk92709540][bookmark: _Hlk92708884]Figure S2. Schematic of pool water treatment process sequence with chemical dosing points and locations of pool water sampling locations. 
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[bookmark: _Hlk92446600]Figure S3. Water sampling and NEMo locations in the studied pool facility. Water samples were collected from roughly 20 cm below the water surface.
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Figure S4. Time-course monitoring of Relative Humidity (RH) at the studied pool facility. Blue line represents the RH measurements. Black horizontal line represents the 60% threshold and red horizontal line represents the 30% threshold. 
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